Supplementary material



Supplementary Fig. 1. The Plastic Teflon & the Glass slide placed at the Stainless-steel mold with the composite packed.

A group of white circles on a black surface

Description automatically generated

Supplementary Fig. 2. Specimens after polishing and ready for baseline color measurement.


A group of rolls of tape

Description automatically generated

Supplementary Fig. 3. Putty mold used to hold the specimens in place.



Supplementary Fig. 4. Soft toothbrushes mounted on the toothbrush simulator machine (ZM-3.12, SD Mechatronik GmbH, Germany).



Supplementary Fig. 5. (A) Specimen #45—Scanning in 12 0’clock position, (B) Specimen #45 - Scanning in 12:15 position. (C) Specimen #45—Scanning in 12:30 position, (D) Color coordinate L\*, a\* and b\* measurements of specimen by spectrophotometer.